{"text_format":"2","workbook":"xls","n_sheets":10,"sheets":["Instructions 1","Instructions 2","Worksheet A","Worksheet B","Worksheet C","T-1","T-2","T-3","T-4","T-5"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":1,"defined_names":9,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Instructions 1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Instructions 2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Worksheet A","index":2,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["STATION CALL SIGN: ",null,null,null,"COMPLETED BY: ",null,null,null,"DATE: "]
["ADDRESS: ",{"$nulls":7},"COUNTY: "]
["ANTENNA","BAND","ANTENNA","FEED LINE","FEED LINE","TRANSMIT","FEED LINE","FEED LINE","POWER","POWER","ANTENNA","POWER"]
["DESCRIPTION","USED","HEIGHT","TYPE","LENGTH","POWER","db LOSS","LOSS","LOST","LOST","POWER","LIMITS"]
[null,null,"(FEET)",null,"(FEET)","(WATTS)","(100 FT)","(db)","(%)","(WATTS)","(WATTS)","(WATTS)"]
["(A)","(B)","(C)","(D)","(E)","(F)","(G)   T-1","(H)","(J)   T-2","(K)","(L)","(M)   T-3"]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]
[{"$nulls":7},0,0,0,""]

{"sheet":"Worksheet B","index":3,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,0,1,10]],"flags":["formulas_cached_only"]}
["STATION CALL SIGN: ",null,null,null,"COMPLETED BY: ",null,null,null,"DATE: "]
["COMPLETE THIS WORKSHEET FOR ALL ROWS ON WORKSHEET 'A' WHERE (L) EXCEEDS (M)"]
["ANTENNA","BAND","ANTENNA","ANTENNA","OPERATING ","DUTY","CONTROL","UNCONTROL","CONTROL","UNCONTROL","POWER"]
["DESCRIPTION","USED","HEIGHT","POWER","MODE","FACTOR","PERIOD","PERIOD","AVG. POWER","AVG. POWER","LIMITS"]
[null,null,"(FEET)","(WATTS)",null,"(%)","(%)","(%)","(WATTS)","(WATTS)","(WATTS)"]
["(A)","(B)","(C)","(L)","(N)","(P)   T-4","(Q)","(R)","(S)","(T)","(M)"]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]
[{"$nulls":8},0,0]

{"sheet":"Worksheet C","index":4,"n_rows":6,"n_cols":10,"rows_kept":6,"cut":false,"hidden":false,"merged":[[1,0,1,9]],"flags":["formulas_cached_only"]}
["STATION CALL SIGN: ",null,null,null,"COMPLETED BY: ",null,null,"DATE: "]
["COMPLETE THIS WORKSHEET FOR ALL ROWS ON WORKSHEET 'B' WHERE (S) OR (T) EXCEEDS (M)"]
["ANTENNA","BAND","ANTENNA","OPERATING ","AVERAGE","LOCATION","ANTENNA","MINIMUM","ACTUAL","SEE"]
["DESCRIPTION","USED","HEIGHT","MODE","POWER","TYPE","GAIN ","DISTANCE","DISTANCE","NOTE"]
[null,null,"(FEET)",null,"(WATTS)",null,"(dbi)","(FEET)","(FEET)"]
["(A)","(B)","(C)","(N)","(S)  OR  (T)","(U)","(V)","(W)   T-5","(X)","(Y)"]

{"sheet":"T-1","index":5,"n_rows":19,"n_cols":11,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,0,0,10]],"flags":["formulas_cached_only"]}
["TABLE 1 - FEED LINE LOSS  (dB / 100 feet)"]
["BAND","RG-174","RG-58","RG-59","RG-8X","RG-213","RG-8 ","9913F7",9913,"1/2\" Dia","450 Ohm"]
[null,"SubMini","Mini","Mini","Mini","Std NC","Std","Ll Flex","Lw Loss","Heliax","Ladder"]
["160 m",1.04,0.47,0.4,0.37,0.26,0.23,0.19,0.16,0.09,0.04]
["80 m",1.46,0.65,0.56,0.52,0.36,0.32,0.26,0.23,0.12,0.05]
["60 m",1.8,0.81,0.69,0.65,0.45,0.4,0.33,0.28,0.15,0.06]
["40 m",2.08,0.93,0.79,0.75,0.52,0.46,0.37,0.32,0.17,0.07]
["30 m",2.52,1.13,0.96,0.91,0.63,0.56,0.45,0.39,0.21,0.09]
["20 m",2.98,1.33,1.13,1.09,0.74,0.66,0.53,0.46,0.24,0.11]
["17 m",3.41,1.52,1.29,1.25,0.85,0.76,0.6,0.53,0.28,0.12]
["15 m",3.69,1.65,1.39,1.35,0.92,0.82,0.65,0.57,0.3,0.13]
["12 m",4.04,1.8,1.52,1.49,1,0.9,0.71,0.62,0.33,0.14]
["10 m",4.3,1.92,1.61,1.58,1.07,0.95,0.75,0.66,0.35,0.15]
["6 m",5.86,2.61,2.17,2.19,1.45,1.3,1.01,0.89,0.46,0.2]
["2 m",10.52,4.65,3.77,4.05,2.59,2.32,1.73,1.54,0.8,0.36]
["1.25  m",13.4,5.9,4.72,5.25,3.29,2.96,2.15,1.93,1,0.46]
["70 cm",20.18,8.83,6.86,8.16,4.93,4.45,3.08,2.82,1.43,0.68]
["33 cm",31.49,13.67,10.23,13.24,7.65,6.92,4.5,4.21,2.1,1.03]
["23 cm",38.67,16.71,12.26,16.57,9.37,8.49,5.34,5.06,2.5,1.25]

{"sheet":"T-2","index":6,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[[0,0,0,4]],"flags":["formulas_cached_only"]}
["TABLE 2 - dB to DECIMAL LOSSES"]
["dB","Loss %",null,"dB","Loss %"]
[0,0,null,2.6,45.05]
[0.1,2.28,null,2.7,46.3]
[0.2,4.5,null,2.8,47.52]
[0.3,6.67,null,2.9,48.71]
[0.4,8.8,null,3,49.88]
[0.5,10.88,null,3.5,55.33]
[0.6,12.9,null,4,60.19]
[0.7,14.89,null,4.5,64.52]
[0.8,16.32,null,5,68.38]
[0.9,18.72,null,5.5,71.82]
[1,20.57,null,6,74.88]
[1.1,22.38,null,6.5,77.61]
[1.2,24.14,null,7,80.05]
[1.3,25.87,null,7.5,82.22]
[1.4,27.56,null,8,84.15]
[1.5,29.21,null,8.5,85.87]
[1.6,30.82,null,9,87.41]
[1.7,32.39,null,9.5,88.78]
[1.8,33.93,null,10,90]
[1.9,35.43,null,12,93.69]
[2,36.9,null,15,96.84]
[2.1,38.34,null,20,99]
[2.2,39.74,null,25,99.69]
[2.3,41.12,null,30,99.9]
[2.4,42.46,null,35,99.97]
[2.5,43.77,null,40,99.99]

{"sheet":"T-3","index":7,"n_rows":28,"n_cols":2,"rows_kept":28,"cut":false,"hidden":false,"merged":[[0,0,0,1],[22,0,22,1],[23,0,23,1]],"flags":["formulas_cached_only"]}
["TABLE  3  -  POWER EXCLUSION"]
["WAVELENGTH","POWER INPUT"]
["BAND","TO THE ANTENNA"]
["160 m","500 watts"]
[" 80 m","500 watts"]
[" 60 m","50 watts"]
[" 40 m","500 watts"]
[" 30 m","425 watts"]
[" 20 m","225 watts"]
[" 17 m","125 watts"]
[" 15 m","100 watts"]
[" 12 m","  75 watts"]
[" 10 m","  50 watts"]
["   6 m","  50 watts"]
["   2 m","  50 watts"]
["1.25 m","  50 watts"]
["70 cm","  70 watts"]
["33 cm","150 watts"]
["23 cm","200 watts"]
["13 cm","250 watts"]
["SHF","250 watts"]
["EHF","250 watts"]
[]
["Repeater stations - ALL Bands"]
["Non-building mounted antennas:  Height above"]
["ground level to lowest point of antenna < 10 meters"]
["and power > 500 w ERP"]
["Building mounted antennas:  Power > 500 w ERP"]

{"sheet":"T-4","index":8,"n_rows":16,"n_cols":8,"rows_kept":16,"cut":false,"hidden":false,"merged":[[15,4,15,6],[10,4,10,6],[11,4,11,6],[12,4,12,6],[13,4,13,6],[15,7,15,9],[15,1,15,3],[1,1,1,9],[3,4,3,6],[4,4,4,6],[5,4,5,6],[6,4,6,6],[7,4,7,6],[8,4,8,6],[9,4,9,6],[14,1,14,3],[7,7,7,9],[8,7,8,9],[9,7,9,9],[10,7,10,9],[11,7,11,9],[12,7,12,9],[13,7,13,9],[14,7,14,9],[14,4,14,6],[10,1,10,3],[11,1,11,3],[12,1,12,3],[13,1,13,3],[6,1,6,3],[7,1,7,3],[8,1,8,3],[9,1,9,3],[4,7,4,9],[5,7,5,9],[6,7,6,9],[2,1,2,3],[2,4,2,6],[2,7,2,9],[3,7,3,9],[3,1,3,3],[4,1,4,3],[5,1,5,3]],"flags":["formulas_cached_only"]}
[]
[null,"TABLE 4 - MODE DUTY FACTOR"]
[null,"TRANSMISSION MODE",null,null,"DUTY CYCLE",null,null,"NOTES"]
[null,"Conversational SSB",null,null,0.2,null,null,"No speech processing"]
[null,"Conversational SSB",null,null,0.4,null,null,"Heavy speech processed"]
[null,"SSB AFSK",null,null,1]
[null,"SSB SSTV",null,null,1]
[null,"AM 50% modulation",null,null,0.5,null,null,"Full carrier DSB modulation"]
[null,"AM 100% modulation",null,null,0.25,null,null,"Full carrier DSB modulation"]
[null,"AM no modulation",null,null,1]
[null,"FM Voice",null,null,1]
[null,"FM Digital",null,null,1]
[null,"ATV video w/image",null,null,0.6]
[null,"ATV video, black screen",null,null,0.8]
[null,"Conversational CW",null,null,0.4]
[null,"Carrier ",null,null,1,null,null,"Used for tune-up purposes"]

{"sheet":"T-5","index":9,"n_rows":46,"n_cols":10,"rows_kept":46,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,2,1,3],[1,4,1,5],[1,6,1,7],[1,8,1,9]],"flags":["formulas_cached_only"]}
["TABLE 5 - DISTANCE FROM ANTENNA (feet)"]
["BAND","GAIN","100 W",null,"500 W",null,"1000 W",null,"1500 W"]
[null,"dBi","CON","UNC","CON","UNC","CON","UNC","CON","UNC"]
["160 m",0,0.5,0.7,1,1.6,1.5,2.2,1.8,2.7]
[null,3,0.7,1,1.5,2.2,2.1,3.1,2.6,3.8]
["80 m",0,0.6,1.4,1.4,3.1,2,4.4,2.4,5.4]
[null,3,0.9,2,2,4.4,2.8,6.2,3.4,7.6]
["40 m",0,1.1,2.5,2.5,5.7,3.6,8.1,4.4,9.9]
[null,3,1.6,3.6,3.6,8,5.1,11.4,6.2,13.9]
[null,6,2.3,5.1,5.1,11.4,7.2,16.1,8.8,19.7]
["30 m",0,1.6,3.5,3.5,7.9,5,11.2,6.1,13.7]
[null,3,2.2,5,5,11.2,7.1,15.8,8.7,19.4]
[null,6,3.2,7.1,7.1,15.8,10,22.4,12.2,27.4]
["20 m",0,2.2,5,5,11.2,7.1,15.8,8.7,19.4]
[null,3,3.2,7.1,7.1,15.8,10,22.4,12.3,27.4]
[null,6,4.5,10,10,22.3,14.1,31.6,17.3,38.7]
[null,9,6.3,14.1,14.1,31.6,20,44.6,24.4,54.7]
["17 m",0,2.8,6.3,6.3,14.2,9,20.1,11,24.6]
[null,3,4,9,9,20,12.7,28.3,15.5,34.7]
[null,6,5.7,12.7,12.7,28.3,17.9,40,21.9,49]
[null,9,8,17.9,17.9,40,25.3,56.5,31,69.2]
["15 m",0,3.3,7.5,7.5,16.7,10.6,23.7,13,29]
[null,3,4.7,10.6,10.6,23.6,15,33.4,18.3,41]
[null,6,6.7,14.9,14.9,33.4,21.1,47.2,25.9,57.9]
[null,9,9.4,21.1,21.1,47.2,29.8,66.7,36.5,81.7]
["12 m",0,3.9,8.7,8.7,19.5,12.3,27.6,15.1,33.8]
[null,3,5.5,12.3,12.3,27.5,17.4,39,21.3,47.7]
[null,6,7.8,17.4,17.4,38.9,24.6,55,31.1,67.4]
[null,9,11,24.6,24.6,55,34.8,77.7,42.6,95.2]
["10 m",0,4.6,10.4,10.4,23.2,14.7,32.8,18,40.1]
[null,3,6.5,14.6,14.6,32.7,20.7,46.3,25.4,56.7]
[null,6,9.2,20.7,20.7,46.2,29.3,65.4,35.8,80.1]
[null,9,13.1,29.2,29.2,65.3,41.3,92.4,50.6,113.2]
["6 m",0,3.3,7.4,4.7,10.5,10.5,23.4,14.8,33.1]
["2 m",3,4.7,10.5,6.6,14.8,14.8,33.1,20.9,46.8]
["1-1/4 m",6,6.6,14.8,9.3,20.9,20.9,46.7,29.5,66.1]
[null,9,9.3,20.9,13.2,29.5,29.5,66,41.7,93.3]
[null,12,13.2,29.5,18.6,41.7,41.7,93.2,59,131.8]
[null,15,18.6,41.6,26.3,58.9,58.9,131.7,83.3,186.2]
[null,20,33.1,74,46.8,104.7,104.7,234.1,148.1,331.1]
["70 cm",0,2.8,6.3,4,8.8,8.8,19.8,12.5,28]
[null,3,4,8.8,5.6,12.5,12.5,28,17.7,39.5]
[null,6,5.6,12.5,7.9,17.7,17.7,39.5,25,55.8]
[null,9,7.9,17.6,11.2,24.9,24.9,55.8,35.3,78.9]
[null,12,11.1,24.9,15.8,35.2,35.2,78.8,49.8,111.4]
[null,15,15.7,35.2,22.3,49.8,49.8,111.3,70.4,157.4]